Ground each of these connections through a separate wire to the star ground on your chassis. The two shown on the card (Input and Output Negative) PLUS  pin 1 of your input XLR and the XLR connector body (2 wires), one from your power supply negative, One from your input transformer shield or can and one from your output jack (if you are unbalanced out) negative. Recapping the 2 big capacitors helps too. I know it is a bunch of wires but reducing the hum required each one. When I remove even one the hum comes up a little…
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